For 1990-2009 cars

# REVISE RADIO REMOVE PROCEDURE SERVICE MANUAL REVISION

#### VEHICLES AFFECTED: 1984 Celebrity Models

The following procedure replaces the information on radio removal shown on Page 8C-5 of the 1984 elebrity Citation Shop Manual.

1. Disconnect battery ground cable.

2. Remove steering column trim panel including hush panel.

3. Remove ashtray and ashtray assembly fuse block - separate ashtray assembly from fuse block. Move both for access.

4. Disconnect cigarette lighter and rear defogger switch connectors.

5. remove cigarette lighter.

6. Remove glove box.

7. Remove I.P. centre trim panel attaching nuts (6).

8. Remove trim panel away from I.P. (enough to remove radio).

9. Remove radio.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.