For 1990-2009 cars

# REAR COMPARPMENT LID WEATHERSTRIP SEALER OOZE-OUT

#### MODELS/YEARS: 1981-1983 OMEGA, CUTLASS SUPREME, CUTLASS CIERA, 88, 98 AND TORONADO

A new sealerless deck lid weatherstrip (Part No. 20469449) has been released for service and should be used when correcting conditions of rear compartment lid weatherstrip sealer ooze-out.

The new weatherstrip does not require sealer in the carrier. Only one length of the new weatherstrip will be serviced, therefore, replacement will involve a cut to fit operation.

Should it become necessary to replace a rear compartment lid weatherstrip the following procedure should be used.

1. Remove lid weatherstrip and clean all sealer from flange around entire lid opening.

2. Begin inserting middle of weatherstrip onto gutter flange at the center of the opening between hinges. Be sure weatherstrip is completely seated to flange around entire opening.

3. Cut off any extra material and cement butt ends together using 3M 8011 Black Weatherstrip Adhesive or equivalent.

4. Close lid and check for leaks.

5. Open lid and check for leaks.

6. If leaks occur, remove weatherstrip from flange.

(a) Brush 3M 8011 Black Weatherstrip Adhesive or equivalent on both sides of the flange (pinch weld) completely around opening.

(b) Apply a bead of 3M8011 or equivalent into the new weatherstrip carrier opening (Figure 1). Allow to dry until adhesive becomes tacky (approximately 5 minutes).

(c) Install new weatherstrip to flange and allow a minimum of 3 hours before closing lid.

7. Close lid and retest for water leaks. If water leaks are found, apply additional 3M 8011 or equivalent under weatherstrip outer lip.

#### WARRANTY INFORMATION

Labor Time Trouble Operation Allowance Code --------- --------- ------- T0077 .6 Hr. 92

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.