For 1990-2009 cars

### Removal Procedure

1. Starting at the rear edge, pull the floor carpet retainers upward in order to disengage the retaining clips.
2. Remove the floor carpet retainer (1) from the driver's side.
3. Remove the floor carpet retainer (1) from the passenger's side.

### Installation Procedure

1. Install the floor carpet retainer (1) to the driver's side.
2. Install the floor carpet retainer (1) to the passenger's side.