For 1990-2009 cars

### Removal Procedure

1. Disconnect the CMP sensor harness connector at the sensor.
2. Remove the CMP sensor bolt.
3. Remove the CMP sensor.

### Installation Procedure

Important: Inspect sensor O-ring for wear, cracks or leakage. Replace if necessary. Lubricate new O-ring with engine oil before installing.

1. Install the CMP sensor.
2. Install the CMP sensor bolt.

Tighten
Install the CMP sensor bolt to 8-12 N·m(5-10 lb in).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Connect the sensor harness connector.