For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 37059 Accessory Drive Belt Tensioner Wrench

Caution: To avoid personal injury when rotating the accessory drive belt tensioner, use a tight fitting 13 mm wrench that is at least 46 cm (18 in) long.

Use J 37059 in order to remove the accessory drive belt by rotating the tensioner counter clockwise.

### Installation Procedure

#### Tools Required

J 37059 Accessory Drive Belt Tensioner Wrench

Caution: To avoid personal injury when rotating the accessory drive belt tensioner, use a tight fitting 13 mm wrench that is at least 46 cm (18 in) long.

Use J 37059 in order to install the accessory drive belt by rotating the tensioner counter clockwise.