For 1990-2009 cars

### Removal Procedure

1. Remove the lower window to the down position.
2. Remove the outer belt sealing strip. Refer to Outer Belt Sealing Strip Replacement .
3. Remove the window frame applique. Refer to Door Frame Applique Replacement .
4. Disengage the fasteners (1) from the upper auxiliary sealing strip.
5. Disengage the upper auxiliary sealing strip from the door frame (1).

### Installation Procedure

1. Engage the upper auxiliary sealing strip to the door frame (1).
2. Engage the auxiliary sealing strip fasteners.
3. Install the window frame applique. Refer to Door Frame Applique Replacement .
4. Install the outer belt sealing strip. Refer to Outer Belt Sealing Strip Replacement .