For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the power seats system check? | -- | Go to Step 2 | Go to Power Seats System Check
2 |

1. Ensure that a proper connection of the power seat switch exists.
2. Use a test lamp in order to backprobe the power seat switch between terminal G and terminal H.
3. Move the power seat switch to the forward and back positions.

Does the test lamp light with the switch in both positions?

--

Go to Step 3

Go to Step 4

3 |

1. Use a test lamp in order to backprobe the forward-back motor connector between terminal A and ground.
2. Move the power seat switch to the forward position.

Does the test lamp light?

--

Go to Step 5

Go to Step 6

4 | Replace the power seat switch. Refer to Power Seat Switch Replacement . Is the repair complete? | -- | Go to Power Seats System Check | --
5 |

1. Use a test lamp in order to backprobe the forward-back motor connector between terminal B and ground.
2. Move the power seat switch to the back position.

Does the test lamp light?

--

Go to Step 7

Go to Step 8

6 | Repair the open in CKT 285 between the power seat switch and the forward-back motor. Refer to Wiring Repairs in Wiring Systems. Does the test lamp light? | -- | Go to Power Seats System Check | --
7 | Replace the forward-back motor. Refer to Front Seat Adjuster Motor Replacement . Is the repair complete? | -- | Go to Power Seats System Check | --
8 | Repair the open in CKT 284 between the power seat switch and the forward-back motor. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Seats System Check | --