For 1990-2009 cars

### Removal Procedure

1. Remove the sunshade (1) from the sunshade support.
2. Rotate the sunshade parallel to the door in order to disconnect the sunshade retention clip.
3. Disconnect the electrical connector.
4. Remove the sunshade bezel (2).

### Installation Procedure

1. Install the sunshade bezel (2).
2. Connect the electrical connector.
3. Move the sunshade parallel to the door.
4. Push up on the sunshade and rotate the sunshade toward the front glass in order to connect the retention clip.