For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 | Place the courtesy lamp switch in the ON position. | The courtesy lamps turn on. |

• | Courtesy Lamps Inoperative

• | Courtesy or Dome Lamps Inoperative

2 | Open and close each door one at a time. |

• | The courtesy lamps turn on for approximately 25 seconds.

• | The courtesy lamps fade out each time.

• | Courtesy Lamps Inoperative

• | Courtesy or Dome Lamps Inoperative

3 | Open the IP compartment. | The IP compartment lamp turns on. | Instrument Panel Compartment Lamp Inoperative
4 | Open the rear compartment. | The rear compartment lamp turns on. | Rear Compartment Lamp Inoperative
5 | Turn each rearview mirror lamp switch to the ON position. | The rearview mirror lamps light. | Inside Rearview Mirror Lamp Inoperative
* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.