For 1990-2009 cars

# REMANUFACTURED TBI FUEL INJECTORS (APPLICATION)

REMANUFACTURED FUEL INJECTORS FOR THROTTLE BODY INJECTION (TBI)

1982 TO 1986 2.0L (VIN CODE P), 1.8L (VIN CODE 0), AND 2.5L (VIN CODE R&U)

Remanufactured Fuel Injectors for General Motors vehicles equipped with Throttle Body injection (TBI) will be available from WDDGM on March 1, 1986. The remanufactured injectors will cover all GM vehicles with single point and dual point TBI for modal years 1980-1986. Refer to Application Chart.

Order placed after March 1, 1986 should be for the remanufactured injectors, however, new injection in dealership inventory may be used until depleted.

To assure that the core injectors are returned in good condition, a two-tube package is used. Refer to Figure 1. The inner tube contains the injector and all of the additional parts and instructions necessary to install the remanufactured injector. The outside tubs must be used to return the old injector to obtain core credit.

#### APPLICATION CHART

REMANUFACTURED CORRESPONDING INJECTOR NEW INJECTOR APPLICATION SERVICE KIT SERVICE KIT Model Year, Engine Sources, Engine V.1. ----------- ------------ --------------------------------------- 17111695 17079694 1983-86 Chevrolet 2.0 P

17111549 17078273 1982-86 Pontiac 1.8 0

17111544 17068993 1982-86 Pontiac 2.5 R or U

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.