For 1990-2009 cars

# RATTLE/BUZZ FROM I/P DURING BRAKE APPLY AND RELEASE

#### MODELS/YEARS 1987-88 FIRENZA, 1989-90 CUTLASS CALAIS AND CUTLASS CIERA MODELS

#### NOTE: This bulletin cancels and supercedes Oldsmobile Dealer Technical Bulletin 89-T-37 (corp. number 975002) which may be discarded. It is being revised to:

- Change part numbers due to a new noise concern with the 18016299 check valve

- Include 1990 model vehicles

- Include Cutlass Ciera models with any engine (previously just included Cutlass Ciera models with 2.5L - VIN R engines).

On some 1987-90 Firenza, Cutlass Calais and Cutlass Ciera models, customers may comment on a rattle or buzz type noise that seems to come from the instrument panel area in front of the driver. The noise is most likely to occur during brake apply or release, during low speed or parking lot maneuvers.

To repair this condition, install a new brake booster check valve, Part Number 18012017.

Parts are currently available through GMSPO.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.