For 1990-2009 cars

### Removal Procedure

1. Remove the push pin retainers (1).
2. Pry the door sill trim plate (2) upward using a flat bladed tool.
3. Clean the tape (4) from the door sill.
4. If you are reusing the trim plate, clean the door sill trim plate (2).

### Installation Procedure

1. Install 2 - sided tape (4) to the door sill trim plate (2).
2. Install the door sill trim plate (2).
3. Install the push pin retainers (1).