For 1990-2009 cars

# RADIO TELEPHONE/MOBILE RADIO INSTALLATION GUIDELINES

#### MODELS/YEARS 1980-1990 MODELS

This bulletin supersedes Dealer Management 86-1-23 with updated information.

The purpose of this bulletin is to make available to dealer personnel radio telephone/mobile radio installation guidelines. This information should be used by dealer personnel in reviewing the mobile equipment users' concerns if a vehicle-transceiver malfunction should occur. This information may be copied and given to the owner and/or installer for their use.

Certain radio telephones or land mobile radios or the way in which they are installed may adversely affect the vehicle operations such as the performance of the engine and driver information, entertainment and electrical charging systems. Expenses incurred to protect the vehicle systems from any adverse effect of any such installation are not the responsibility of General Motors Corporation. The following are general guidelines for installing a radio telephone or land mobile radio in General Motors vehicles. These guidelines for installing a radio telephone or land mobile radio in General Motors vehicles. These guidelines are intended to supplement, but not to be used in place of, detailed instructions for such installations which are the sole responsibility of the manufacturer of the involved radio telephone or land mobile radio.

INSTALLATION GUIDELINE (refer to the enclosed figures during installation)

1. Transmitter Location

A. Locate transceiver for remote radios on driver's side of trunk as near to the vehicle body side as possible.

B. One piece transceivers should be mounted under dash or on transmission hump where they will not interfere with vehicle controls or passenger movement.

2. Antenna Installation

A. The antenna should be a permanent-mount type located in the center of the roof or center of the rear deck lid. Glass mounted antennas should be kept as high as possible in the center of the rear window or windshield. If a magnetic-mount antenna must be used, care should be taken to mount the antenna in the same location as a permanent mount type. If a disguise-mount antenna is used, great care should be taken to shield the tuning network from vehicle electronics and wiring, or to mount the tuning network in an area completely clear of vehicle electronics and wiring.

B. Each vehicle model and body style reacts to radio frequency energy differently. When dealing with an unfamiliar vehicle, it is suggested that a magnetic-mount antenna be used to check the proposed antenna location for unwanted effects on the vehicle. Antenna location is a major factor in these effects.

3. Antenna Cable Routing

A. Always use a high quality coax (at least 95% shield coverage) routed away from the Engine Control Module (ECM) and other electronics modules.

B. Care should be taken to avoid routing feedline with any vehicle wiring.

4. Antenna Tuning

A. It is important that the antenna be tuned properly and reflected power be kept to a minimum. (VSWR( 2:1)

5. Radio Wiring and Connection Locations

A. Transceiver Power Leads:

These connections should be made directly to the battery itself, in- cluding the ground, or to the jump start block on vehicles so equipped. The transceiver power feeds should be #10 AWG wire or larger, twisted if possible. The ground wire should not be attached to the body at any point. Appropriate in-line fuses for both the positive and ground leads should be located as near the battery as possible.

#### NOTE: It is recommended that a fuse be placed in the transceiver ground lead to prevent possible damage to the transceiver, in the event the battery to engine-block ground is inadvertently disconnected.

For ONE-PIECE TRANSCEIVERS where ignition switch control is desired, a 12 v power contactor must be installed in the transceiver positive lead. The contactor should be located at the vehicle battery with the coil of the contactor driven through an appropriate in-line fuse from an available accessory circuit or ignition circuit not powered during cranking. The coil of the contactor must return to battery negative.

B. Handset or Control Unit Battery and Ground:

Any ground lead from a handset or control unit must return to battery negative. It is preferable that the positive lead for a handset or control unit be connected directly to the battery. It is recommended that the handset or control unit positive and ground leads be appropriately fused separately from the transceiver positive and ground leads. If ignition switch control is desired, the handset or control unit positive lead may be connected through an appropriate in-line fuse to an available accessory circuit or ignition circuit not powered during cranking.

C. Connections for Multiple Transceivers and Receivers:

If multiple transceivers or receivers are to be installed in the vehicle, power leads to the trunk or under dash should be terminated in covered insulated buss bars. All transceivers or receivers may then have their power leads connected to the buss bars. This makes a neater installation and reduces the number of wires running to vehicle underhood.

6. Wire Routing

A. The power leads should be brought through a grommet on the driver's side firewall. For trunk-mounted transceivers, the cables should con- tinue on along the driver's side door sills, under the rear seat, and into the trunk through the rear bulkhead. If the battery is located on the passenger side, battery leads should cross the vehicle in front of the engine. All attempts should be made to maintain as much distance as possible between radio power leads and vehicle electronic modules and wiring.

B. For police vehicles, radio power leads should be routed in the conduit provided with the option package.

7. Troubleshooting

A. Should vehicle problems develop following installation, the source of the problem should be determined prior to further operation of the vehicle.

B. Possible causes of vehicle problems include:

1. Power feeds connected to points other than the battery.

2. Antenna location.

3. Transceiver wiring located too close to vehicle electronic modules or wiring.

4. Poor shielding or poor connectors on antenna feedline.

8. Contact and Feedback

A. GM vehicles have been designed and extensively tested for immunity to known sources of RF energy. However, it is impossible to test for every combination of RF sources and installations. If a persistent condition is encountered,

#### WRITE TO:

EMC DEPT. - MR BLDG 40 GENERAL MOTORS PROVING GROUND MILFORD, MICHIGAN 48042-2001

Auxillary Electrical Equipment GM Recommended Installation

AC-Delco Side Terminal Adaptor Package 1846855, when combined with the longer battery bolt and spacer will provide the simple, tight, corrosion resistant connection illustrated. Parts can also be purchased at car dealerships.

AC-DELCO CAR DEALER Item Catalog 7A10 "Parts" Book ---- ------------ ------------- Kit 1846855 1846855 Bolt 7803 12004188 Spacer 7804 12004189

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.