For 1990-2009 cars

# PASSENGER SEAT WILL NOT LOCK INTO POSITION-NEW SEAT SPRING

#### Subject: PASSENGER SEAT WILL NOT LOCK INTO POSITION (REPLACE SEAT OUTER LATCH RETURN SPRING)

#### Model and Year: 1989-91 CUTLASS CALAIS COUPE MODELS

Condition: The standard passenger seat EZ Entry seat adjuster for 1989 through early 1991 Cutlass Calais coupe models may exhibit a no-lock condition when repositioning the seat assembly forward or backward.

Cause: The latch return spring on the outer track of the seat adjuster may break when adjusting the seat assembly forward or backward. Once the spring is broken, the latch on the outer track cannot return to the lock position.

Correction: Replace passenger seat outer latch return spring as follows:

#### Remove or Disconnect:

1. Seat adjuster trim covers. 2. Seat adjuster-to-floor pan attaching nuts, then remove seat assembly from vehicle. 3. Outer latch return spring from latch and track (Figure 1).

#### Install or Connect:

1. Outer latch return spring, P/N 12510770 to latch and track (Figure 1). 2. Seat assembly into vehicle and install seat adjuster-to-floor pan attaching nuts. Tighten nuts to 29 N.m. (21 lbs. ft.). 3. Seat adjuster trim covers.

Parts are currently available from GMSPO.

Labor Operation Number: T1730 Labor Time: .3 Hour

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.