For 1990-2009 cars

### Removal Procedure

1. Disconnect the cruise control cable tab from the throttle body injection (TBI) cam (6). Rotate the TBI cam to ¼ open throttle in order to release the tab.
2. In order to release the cable (4), push the locating fitting inward and pull the unit free from the throttle bracket (2).
3. Remove the cable assembly (4) from the module (3) by turning the cable assembly ¼ turn counterclockwise.
4. Remove the cable from the ribbon.
5. Remove the cable (3) from the retaining clips (1).

### Installation Procedure

1. Install the cable (3) to the retaining clips (1).
2. Install the cable to the ribbon.

Important: Ensure that the ribbon does not become twisted when connecting the cable to the module.

3. Connect the cable assembly (4) to the module (3) by turning the cable assembly ¼ turn clockwise.
4. Install the cruise control cable tab (4) to the TBI cam (6).
5. Align the cruise control cable fitting to the throttle body bracket (1). Snap the fitting into place. Ensure that the fitting is retained.
6. Adjust the cruise control cable. Refer to Cruise Control Cable Adjustment .