For 1990-2009 cars

# WHISTLE NOISE FROM BLOWER - MODIFY BLOWER CASE

#### Models/Years 1990 CUTLASS CALAIS

Some 1990 Cutlass Calais models built between the VIN breakpoints listed below may exhibit a "whistle" noise when the blower is operated under certain conditions. The whistle noise may be experienced under the following operating conditions:

With A/C Without A/C

- High Blower Speed Only - High Blower Speed Only - Max AC Mode - Bi-level Mode - Norm AC Mode - Vent Mode - Bi-level Mode - Temp Lever Set to Full - Vent Mode Cold Position - Temp Lever Set to Full Cold Position

VEHICLES BREAKPOINTS

With AC Without AC Plant Nameplate From VIN # to ViN From VIN # to VIN Lansing Oldsmobile LM748734 - LM759966 LM749377 - LM759966

In order to reduce the whistle noise the following procedure should be used.

1. Remove blower motor and fan assembly from vehicle

2. Locate tab (Figure 1) inside blower motor case

3. Bend tab downward about 20 degrees as shown in Figure 1

4. Install previously removed motor and fan assembly

#### WARRANTY INFORMATION:

With A/C Without A/C

Labor Operation Number: D1322 D1320 Labor Time: 0.4 hour 0.4 hour Trouble Code: 92 92

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.