For 1990-2009 cars

### Removal Procedure

The relays in the illustration are described in the following order:

• |
- The fuel pump relay (1)

• |
- The cooling fan relay 2 (2)

• |
- The cooling fan mode relay (3)

• |
- The cooling fan relay 1 (4)

• |
- The A/C compressor relay (5)

1. Remove the underhood fuse block cover.
2. Remove the appropriate relay.

### Installation Procedure

The relays in the illustration are described in the following order:

• | The fuel pump relay (1)

• | The cooling fan relay 2 (2)

• | The cooling fan mode relay (3)

• | The cooling fan relay 1 (4)

• | The A/C compressor relay (5)

1. Install the appropriate relay.
2. Install the underhood fuse block cover.