For 1990-2009 cars

Caution: The tilt spring and the spring guide are under pressure. The tilt spring and the spring guide may become a projectile. Secure the spring with locking pliers during removal. Secure the spring with locking pliers during installation. Bodily injury may result during removal and installation of the tilt spring and the spring guide. Always use caution during removal and installation of the tilt spring and the spring guide.

1. Remove the tilt spring.

1.1. | Pry the tilt spring up until a bulge occurs and most of the tilt spring tension is removed.

1.2. | Secure the tilt spring with locking pliers and continue prying until the tilt spring disengages from the post of the steering column support assembly.

2. Remove the spring guide (1) from the tilt spring (2).