For 1990-2009 cars

# SERV. MAN. UPD.-SEC.6D STARTER REMOVAL 3300 ENG.

#### MODELS/YEARS 1989-90 CUTLASS CIERA AND CUTLASS CRUISER

The procedure in this bulletin replaces the Starter Motor R&R procedure for the 3.3L engine published in the 1989 and 1990 Service Manuals.

#### Models Affected 1989 Oldsmobile Cutlass Ciera and Cutlass Cruiser at page 6D2-2

1990 Oldsmobile Cutlass Ciera and Cutlass Cruiser at page 6D2-1

#### Procedure:

Remove or Disconnect

1. Negative battery cable.

- Raise the vehicle and suitably support. Refer to General Information (Section OA).

2. Starter motor wiring.

3. Bolts from flywheel cover.

4. Flywheel cover.

5. Bolts from starter motor.

6. Starter motor.

Install or Connect

1. Starter motor.

2. Bolts to starter motor.

Tighten Bolts to 40 N.m (30 lb. ft.)

3. Flywheel cover.

4. Flywheel cover bolts.

Tighten Bolts to 10 N.m (89 lb. in.)

5. Starter motor wiring.

- Lower vehicle

6. Negative battery cable.

Tighten

- Cable to 12 N.m (106 lb. in.)

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.