For 1990-2009 cars

### Removal Procedure

1. Remove the radio. Refer to Radio Replacement .
2. Remove the instrument panel storage compartment. Refer to Instrument Panel Compartment Replacement in Instrument Panel, Gauges, and Console.
3. Remove the antenna extension cable retainers (2) from the instrument panel (1).
4. Remove the right side carpet retainer. Refer to Carpet Retainer Replacement in Interior Trim.
5. Pull back the carpet in order to gain access to the antenna extension cable (2). Refer to Front Floor Panel Carpet Replacement in Interior Trim.
6. Disconnect the antenna extension cable (2) from the main body harness (1).
7. Remove the antenna extenson cable (2) from the vehicle.

### Installation Procedure

1. Install the antenna extension cable (2) to the vehicle.
2. Connect the antenna extension cable (2) to the main body harness (1).
3. Reposition the carpet. Refer to Front Floor Panel Carpet Replacement in Interior Trim.
4. Install the right side carpet retainer. Refer to Carpet Retainer Replacement in Interior Trim.
5. Install the antenna extension cable rosebud retainers (2) to the instrument panel (1).
6. Install the instrument panel storage compartment. Refer to Instrument Panel Compartment Replacement in Instrument Panel, Gauges and Console.
7. Install the radio. Refer to Radio Replacement .