For 1990-2009 cars

Table 1: | Program Connector
Table 2: | Remote Control Door Lock Receiver

#### Program Connector

Connector Part Information |

• | 12047663

• | 2-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK/WHT | 1455 | Keyless Entry Program Enable Signal
B | BLK | 850 | Ground

#### Remote Control Door Lock Receiver

Connector Part Information |

• | 12129431

• | 16-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 694 | Power Door Lock Motor Feed, Driver Door (UNLOCK)
B | WHT | 194 | PowKer Door Lock Relay Feed, UNLOCK
C | BLK | 28 | Horn Relay Output
D | LT BLU | 395 | Door Handle Switch Signal, Right Front
E-F | -- | -- | Not Used
G | BLK/WHT | 56 | Trunk Release Motor Feed
H | GRY | 382 | Trunk Release Enalbe Relay Output, Common Contact
J-K | -- | -- | Not Used
L | BLK/WHT | 1455 | Keyless Entry Program Enable Signal
M | YEL | 1737 | Transaxle Mounted Neutral Safety Switch Output
N | BLK | 850 | Ground
P | ORN | 1040 | Fuse Output, Battery (Type III Fuse)
R | LT BLU | 195 | Power Door Lock Relay Feed, LOCK
S | -- | -- | Not Used