For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Door Trim Panel Replacement .
2. Pull up the door inner belt sealing strip in order to disengage the unit from the door flange (1).

### Installation Procedure

1. Push down the door inner belt sealing strip in order to engage the unit to the door flange (1).
2. Install the door trim panel. Refer to Door Trim Panel Replacement .