For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the left splash shield. Refer to Wheelhouse Splash Shield Replacement in Body Front End.
3. Remove the electronic brake control module. Refer to Electronic Brake Control Module Replacement in Antilock Brake System.
4. Remove the electrical connector from the washer pump.
5. Remove the hose from the washer pump.
6. Remove the electrical connector from the solvent level sensor.
7. Remove the 3 screws and the washer solvent container from the vehicle.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the washer solvent container onto the vehicle with the 3 screws.

Tighten
Tighten the 3 screws to 6 N·m (53 lb in).

2. Connect the electrical connector to the solvent level sensor.
3. Connect the hose to the washer pump.
4. Connect the electrical connector to the washer pump.
5. Install the electronic brake control module. Refer to Electronic Brake Control Module Replacement in Antilock Brake System.
6. Install the left splash shield. Refer to Wheelhouse Splash Shield Replacement in Body Front End.
7. Lower the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.