For 1990-2009 cars

### Removal Procedure

1. Disconnect the accelerator and cruise control cables from throttle body lever.
2. Depress the tangs and remove the accelerator and cruise control cables from accelerator cable bracket.
3. Remove the nuts and bolts holding the accelerator cable bracket to the throttle body.
4. Remove the accelerator cable bracket.

### Installation Procedure

1. Install the accelerator cable bracket to throttle body.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Reinstall the nuts and bolts.

Tighten

• | Tighten the nuts to 26 N·m (19 lb ft).

• | Tighten the bolts to 12 N·m (106 lb in).

3. Connect the accelerator cable into accelerator cable bracket.
4. Connect the accelerator cable cross slug to the throttle body slots.
5. Connect the cruise control cable into accelerator cable bracket.
6. Connect the cruise control cable to the throttle body lever.