For 1990-2009 cars

### Removal Procedure

1. Remove the purge valve electrical connector.
2. Remove the hoses to the purge valve.
3. Remove the purge valve from the mounting bracket.
4. When replacing the bracket, remove the purge valve mounting bracket attaching nut.
5. Remove the purge valve mounting bracket.

### Installation Procedure

1. Install the purge valve mounting bracket and the attaching nut.

Tighten
Tighten the purge valve mounting bracket attaching nut to 6-10 N·m (53-88 lb in).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Slide the purge valve into the mounting bracket.
3. Install the hoses to the purge valve.
4. Install the valve electrical connector.