For 1990-2009 cars

### Disassembly Procedure

#### Tools Required

• | J 22888 Puller

• | J 23598 Pilot

• | J 22888-30 Puller Legs

1. Remove the left differential side bearing using the J 22888 , the J 22888-30 and the J 23598 .
2. Remove the differential ring gear bolts from the differential case.
3. Remove the differential ring gear from the differential case.
4. Remove the right differential side bearing using the J 22888 ,J 22888-30 and the J 23598 .
5. Remove the vehicle speed sensor (VSS) ring using the J 22888 ,J 22888-30 and the J 23598 .
6. Remove the following parts:

• | The pinion shaft roll pin

• | The pinion shaft

• | The pinion gears

• | The pinion gear thrust washers

• | The side gears

• | The side gear thrust washers