For 1990-2009 cars

### Removal Procedure

1. Turn OFF the ignition switch.
2. Disconnect the Intake Air Temperature (IAT) sensor electrical connector.
3. Disconnect the MAF sensor electrical connector.
4. Remove the air inlet duct from the MAF sensor and the throttle body.
5. Remove the MAF sensor from the air filter housing.

### Installation Procedure

1. Install the MAP sensor to the bracket.
2. Connect the MAP inlet vacuum hose.
3. Connect the MAP sensor electrical connector.