For 1990-2009 cars

### Removal Procedure

1. Remove the split/folding rear seat back. Refer to Rear Split Folding Seat Back Replacement .
2. Place the rear seat back on a surface that meets the following conditions:

• | Clean

• | Dry

• | Non-abrasive

3. Remove the center folding armrest.
4. Separate the pad and the cover from the rear seat back frame.
5. Remove the cover from the pad. Disengage the tie straps.

### Installation Procedure

1. Install the cover to the pad. Engage the tie straps
2. Install the pad and the cover to the rear seat back frame.
3. Install the center folding armrest.
4. Install the split/folding rear seat back. Refer to Rear Split Folding Seat Back Replacement .