For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 |

1. Drive the vehicle above 40 km/h (25 mph).
2. Depress and release the cruise ON/OFF button.
3. Depress the cruise control SET/COAST button and then release the button.
4. Release the accelerator pedal.

The CRUISE indicator lights and the vehicle maintains a set speed.

Cruise Control Inoperative

2 |

1. Depress the cruise control RES/ACCEL switch and hold the switch until the vehicle speed increases by 6.4-8.0 km/h (4-5 mph).
2. Release the cruise control RESUME/ACCEL switch.

The vehicle accelerates and maintains the new higher set speed.

Cruise Control Inoperative

3 |

1. Depress the cruise control SET/COAST switch and hold the switch in position until the vehicle speed decreases by 6.4-8.0 km/h (4-5 mph).
2. Release the cruise control SET/COAST switch.

The vehicle decelerates and maintains the new lower speed when the speed is above 40 km/h (25 mph).

Cruise Control Inoperative

4 | Depress the cruise ON/OFF button. | The cruise control disengages. (The memory is unchanged) | Cruise Control Inoperative
5 | Press the brake pedal lightly. | The cruise control disengages. (The memory is unchanged) | Cruise Control Inoperative
6 | Depress the cruise control RESUME/ACCEL button. | The vehicle accelerates to, and then maintains, the previously set speed. | Cruise Control Inoperative
7 | Press and quickly release the cruise control switch RESUME/ACCEL button once (tap-up). | The vehicle speed increases by approximately 1.6 km/h (1 mph) and maintains the new set speed. | Cruise Control Inoperative
8 | Press and quickly release the cruise control SET/COAST button once (tap-down). | The vehicle speed decreases by approximately 1.6 km/h (1 mph) and maintains the new set speed. | Cruise Control Inoperative