For 1990-2009 cars

# UPDATE-MANUAL TRANSAXLE ON-CARSERVICING

#### MODELS/YEARS 1990 CUTLASS CALAIS AND CUTLASS SUPREME

This bulletin supplements the procedure outlined in the appropriate service manuals on the following pages:

Cutlass Calais - Page 7B-14 Cutlass Supreme - Page 7B-20

Prior to disconnecting the transaxle from the engine, the throttle body coolant pipes must be removed. The throttle body coolant pipes must never be bent to gain clearance. Removal of the throttle body coolant pipes is found in Section 6B of the service manual.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.