For 1990-2009 cars

# FRENCH LABEL INSTALLATION INSTRUCTIONS

#### SUBJECT: 1992 FRENCH LABEL INSTALLATION INSTRUCTIONS

I. Passenger Cars - Page 1 II. Light Duty Trucks (Diesel Only) - Page 14 III. Light Duty Trucks - Page 16 IV. Medium Duty Truck (C5-6-7, W4-5-7) - Page 23

I. VEHICLES AFFECTED: All 1992 Passenger Cars ---------------------------------------------- Labels are pressure sensitive, therefore, surfaces must be clean, dry, warm and free of contaminants, before labels are affixed. Labels must be pressed firmly over their entire surface. Locate labels next to corresponding English labels, unless otherwise noted. Both labels must be readable.

#### Engine

1) Fan Caution Label - If vehicle is equipped with an English label, place a French label over it. Otherwise, place label adjacent to the English embossed message on fan shroud. - For B, C, H or F-car use 52350076. otherwise use label 52355271. - For Saturn, use 52363687

2) Battery Heat Shield Label. - Use label 52363413 on the W-car adjacent to English label.

3) Battery Caution Labels

For Battery No. 1981733 place label 52363359 on C,H cars For Battery No. 1981730 place label 52363361 on A,B,F,U,L For Battery No. 1981735 place label 52363362 on B,C,H For Battery NO. 1981731 place label 52363363 on F cars For Battery No. 1981601 place label 52363364 on A,C,H,F,J,N.L For Battery No. 1981818 place label 52363365 on W cars For Battery No. 1981763 place label 52363367 on C,H,V,K,E,D Place label 52362567 on M car Place label 52363366 on w car Place label 52363441 (L98) or 442 (LT5) on Y

4) Battery Charge Indicator Label - Place 52362565 over the English label on M car.

5) Air Conditioner Compressor/Evaporator Labels - Place 744775 on: A,B,C,H,V,K,E,D,F,J,N. - Place Label 744775 over the words "Refrigerant Oil, Model No.", such that LH edge of overlay is even with LH edge of silver portion of compressor label. - Place label 52360150 on: Optima T adjacent to English. label.

6) Turbo Engine Oil Recommendations Label - Place 52362528 on J,N adjacent to English label

7) Hood Prop Rod Label - Place label 52354520 over English label on: L,T cars. - Place label 52364164 over English label on: U car.

8) Engine Oil Fill Cap Label - Place labels 52355864 or 52355865 (depending on which oil is used, SW or low) over English label on: A, B, C, H, V, K, E, D, F, U, J, N, L, W cars.

9) Accessory Belt Routing Label - The Bilingual label should go directly over top of the English label so that the Bilingual Only shows.

For U.S. No. 10042993 use 52356183 on A For U.S. No. 14076368 Use 52356802 on J,N.L For U.S. No. 10044858 Use 52356837 on A,W,U,J,N,L For U.S. No. 10045371 Use 52356812 on C,H,V,K,D,E For U.S. No. 10045365 Use 52356815 on C,H,V,K,E,D For U.S. No. 10045372 Use 52356813 on C,H,V,K,E,D For U.S. No. 10045326 Use 52356814 on C,H,V,K,E,D For U.S. No. 10045063 Use 52356860 on J,N For U.S. No. 10105211 Use 52361696 on V,K,D,E For U.S. No. 10100036 Use 52361585 on F For U.S. No. 22518472,3,4 and 1627187 Use 52352960 on C,H,A For U.S. No. 10055889 Use 52360073 on B,F For U.S. No. 25523397 Use 52354640 on J,N For U.S. No. 14092380 Use 52355272 on Y For U.S. No. 10116294 Use 52363422 on J,N For U.S. No. 10186176 Use 52364151 on Y (LT1) For U.S. No. 21006214 Use 52363686 on Saturn For U.S. No. 10114996 Use 52364109 on W

10) Vehicle Fluids Identification Label - Place label 52353412 beside the English label on top of the air cleaner on C,H,V,K,D,E.

11) A/C Refrigerant Charging Procedure Label - Place label 52353413 over the original English label on top of the radiator support on: C,H. - Place label 52355251 adjacent to English label on: V,K,E,D. - Place label 52356186 adjacent to English label on: J,N.L. - Place label 52362997 adjacent to English label on U car.

12) Refrigerant Caution Label - Place label 52361685 adjacent to English label on L. - Place label 52360351 adjacent to English label on W.

13) Composite Headlamp Label - Place label 52355512 adjacent to English label on: A, C, H, V, K, E, D, F, J, N, T cars.

14) Fuse Block Identification Label - Place label 52355488 over the existing English label on: V,K,E,D. - Place label 52363378 over the existing English label on W car.

15) Relay Centre Label - Place labels 52355500, or 52355504 over existing English labels on: V,K,E,D.

16) Caution Wiper Label - Place label 52362755 adjacent to the existing English label on U car.

17) Battery Catalogue Number - Place 52356160 on A,B,C,H,V,K,D,E,F,J,N,L.

18) Notice Electrical System Ignition "Off" Warning - Place label 52356803 over existing English label on B, C, H, V, K, D, E

19) Special Coolant fill Label - Place 52360259 adjacent to existing English label on W.

20) HDLP Bulb Replacement Instruction Label - Place label 52356207 adjacent to English label on J and N.

21) Inflatable Restraint System Label - Place label 52360625 adjacent to English label on C,H. - Place label 52362998 adjacent to English label on B. - Place label 52362515 adjacent to English label on F - Place label 52363003 adjacent to English label on L - Place label 52362834 adjacent to English label on Y

22) Brake Fluid Pressure Caution Label - Place 52361684 on: adjacent to English label A,C,H,V,K,D,E.

23) Notice Dexron II Only Label - Place 52362564 on: adjacent to English label M.

24) Caution Active Ride Suspension Label - Place 52362571 adjacent to English label 10140793 on: V,K,D,E.

25) Caution Frt. Susp. Gas Under Pressure Label - Place 52362570 adjacent to English label on: V,K,D,E.

26) Caution Fuel Flammable Label - Wrap four (4) 52362963 labels on all vehicles around fuel line adjacent to English label. If no English labels present, there is no need to use the French.

27) S.I.R. Caution Labels - Place three (3) 52363000 on B,C,H,V,K,E,D,F,M,L,Y Saab 1 on pass.dr. pillar, 1 on underside of steering column, 1 on rad supt. bar underhood.

28) Engine Jump Start Label - Place 52364147 adjacent to English label

29) Diesel Service Label - Use 52364127 adjacent to English label 10149667

#### Passenger Compartment

1) Owner's Manual Reference Label - Place label 745764 on trailing edge of door adjacent to Tire and Certification Labels on: A, B, C, H, V, K, E, D, F, U, J, N, M, L, T, R, W, Y.

2) Shock Absorber Caution Label (4 per vehicle) - Place 52353504 adjacent to English label on V,K,E,D

3) Manual Transmission Shift Indicator Light Label - Place label 52353708 adjacent to English label on LH Sunvisor on: A, F, J, N.

4) Automatic Headlamp Dimmer Sensor - Place 744683 on V,K,E,D

5) Apply Brake to Shift Label - Place 52362974 on C,H,R

6) Roof Panel Notice Label - Place label 52350964 on left and right side roof panels over English labels on: V,K,E,D..

7) Anti-theft (on Window Label)

- Place 52360255 in glove box of vehicle on F.

8) Fuse Block Identification Labels - Remove the fuse block cover and install label 52353407 (Olds), 52353408 (Buick), or 52353409 (Cadillac) on C,H - Place labels 52355486 (Cadillac) and 52355487 (Olds) over existing English label on V,K,E,D - Place label 52360260 over existing English label on L - Place label 52354729 over existing English label on J,N

9) Headlight Flash to Pass Signal Switch Tag - Place tag 52352651 on shaft of signal switch adjacent to English tag on A

10) Interior Light Switch Tag - Place label 52363544 on U

11) Engine and Diesel Engine Start Procedure Label - Place 52362589 on T

12) Instruction Sheet Sunroof Crank Label - Place 52354062 in glove box on B

13) Childproof Lock Label - Place label 52362462 over English label on R - Place label 52363755 over English label on M

14) Dual Mode Retractor Child Restraint Seat Belt Label - Place 52363002 around D-ring side of belt directly around stitched area on A,B,U,J,N,L (2 per job) - Place 20584675 on C,H,M (2 per job)

15) Extension Spare Wheel Stowage Label - Place label 52355166 on Extension adjacent to English label on J,N

16) Relay Centre Label - Place label 52355503 over label 25522931 on: V,K,E,D - Place label 52355501 over label 25522933 on: V,K,E,D

17) Electronic Brake Control Info Tag - Place label 52363424 on Y-car

18) All Wheel Drive or 4-wheel Drive Instruction - Place 52361596 adjacent to existing English label on A,W cars

19) Tire Sensor Label (4 per vehicle) - Place 52356861 adjacent to 14102346 on Y car

20) Radio Theft Deterrent Label - Place 52356797 adjacent to English label if English label is used. Otherwise put in glove box on A car

21) Inflator Instruction Label - Place 52363423 on U car

22) Inflatable Restraint System Label - Place 52362980 on B,C,H,V,K,E,D,F,L,Y

23) Instruction Sheet Hub-Cap Installation - Place 52360389 in glove box on C,H

24) Anti-Theft Locking System Label - Place label 52360256 adjacent to English label on: L,W

25) Caution Seat Code A,B,C - Place label(s) 52362748(2/car),49(2/car),50(1/car) adjacent to English label on U car

26) Scotchguard Label - Place 52364312 on windows of cars with cloth interiors (adjacent to English label) on Chevrolet products

27) Roof Lift Off Windows Storage Instructions (T-Roof) - Place 52362754 adjacent to English label ON F

28) Jack Location Label - Place 52362768 on to English label on Y

29) Notice Remove Fuel Quickly Label - Place 52363424 on B car

30) Door Edge Caution - Place 52363592 (Rt Side) and 52363593 (Lt Side) over existing English labels on U car

31) Anti Lock Brake Label - Place 52364340 adjacent to English message on B car

32) Tag Electronic Brake Control Info - Make sure tag 52363424 is installed and gets to customer

#### Trunk

1) Third Seat Release Label - Place label 744742 beside established label near the release lever on RH side on B wagon

2) Cargo Cover Label - Place 744774 adjacent to English label on A

3) Jack Locator Label - Place 52362568 on M - Place 52361462 over English label on W

4) Wire Wheel Cover Lock Removal Label - Place 746197 adjacent to English label on trunk lid on A,B,V,K,D,E,J,N - Place 52353419 on A,C,H - Place 52361679 on W

5) Roof Panel Stowage Instruction Label - Place label 52354086 on F

6) Inflation Canister Label - Place 746415 on F car

7) Space Saver Spare Tire Label - Place label 52350966 on rim next to original label after removing tire and inflation canister on F car.

8) Jack Assembly Caution Label - Place 746124 over English label on A - Place 52351308 on opposite side of English label on A - Place 52353402 on opposite side of English label on A - Place 52363406 on opposite side of English label on B - Place 52353404 on opposite side of English label on CH - Place 52356209 on jack on F - Place 52354513 opposite to corresponding English label on U - Place 52354509 opposite to corresponding English label on J,N - Place 52362566 on jack on M - Place 52360095 adjacent to English label on T - Place 52354791 adjacent to English label on R - Place 52363383 opposite to corresponding English label on L - Place 52362137 adjacent to English label on W - Place 52363428 on E,V,K - Place 52354515 on Y

9) Jack Instruction Labels - Place 52361461 beside English label after removing the RH quarter panel trim cover on A station wagon - Place 52363372 on B - Place 52361491 adjacent to English label on C (Cad) - Place 52361492 adjacent to English label on C,H (Buick, Olds, Pontiac) - Place 52362586 on F - Place 52362534 on U - Place 52365477 on J,N - Place 52362563 on M - Place 52360094 adjacent to English label on T - Place 52362530 or 52362531 adjacent to English label on - Place 52362936 adjacent to English label on L - Place 52362320 adjacent to English label on W - Place 52362765 on Y - Place 52362766 on Y - Place 52362150 on A - Place 52373371 on B - Place 52361463 on F (stowage) - Place 52361660 adjacent to English label on W - Place 52360710 on A (AWD) - Place 52350162 on D - Place 52360057 on V - Place 52362569 on M (stowage) - Place 52362767 on Y and ZR-l wheel stowage - Place 52363427 on E,K

10) Spare Caution Label (Compact and Regular) - Place 52362142 on A - Place 52353513 on A,B,C,H,V,K,D,E,F,J,N,L,W (Olds excluded) - Place 52353291 on Y

11) Remote Locking Fuel Door Label - Place 52351460 on bumper filler panel adjacent to English label on C,H,V,K,D,E

12) Electric Lock Fuel Cap Label - Place label 52352880 on fuel cap opposite to English label on: B, C, H, V, K, D, E

13) Fuel Filler Door Manual Release Label - Place label 52353416 beside the English label on the inner surface of the rear trunk lid flange on: C,H - Place label 52355250 beside the English label on the inner surface of the rear trunk lid flange on V,K,D,E

14) Jack Instructions Location Label - Place 52353417 on compartment lid adjacent to English label on C,H

15) Notice Convertible Top Close Label - Place 52362930 on F

16) Tailgate Transfer Decal - Place decal 52353624 below the English decal which is located just above the tailgate door lock on A car. (Note: French decal should be positioned below the lock cylinder).

17) Full Size Flat Aluminum Wheel Stowage - Place label 52354613 adjacent to English label on A.

18) Centre Hub Cap Removal Instruction - Place 52354730 adjacent to English label on J,N

19) Trailer Towing Notice Label - Place label 52355167 adjacent to English label on: V,K,D,E.

20) Jack Pad Filler Location - Place 52360931 adjacent to English label on W

21) Amcor Security Lug Nuts - Place 52362957 on A,J,N,L,W

22) Convenience Net Label - Place 52364100 adjacent to English label on B wagons

23) Inflator Operator Instructions - Place 52364163 adjacent to English label

24) Remove and discard all extraneous English advertising.

Labels which are released late will be added to this attachment when the installation instructions are reissued.

II. VEHICLES AFFECTED: 1992 Light Duty Trucks (Diesel Only) ----------------------------------------------------------- General Information -------------------- Labels are pressure sensitive; therefore, surfaces must be clean, dry, warm and free of contaminants, before labels are affixed. Labels must be pressed firmly over the entire surface.

Locate labels next to English labels, unless otherwise noted. Both labels should be readable.

#### Engine Compartment

1) Maximum Voltage Caution Label - Place 52354639 adjacent to English label

2) Oil Filler Cap Label - Place label 52355864, 52355865 over one of the original labels on the oil filler cap. (Key on Oil required)

3) Diesel Fuel Filter Labels - Place label 74944 over English label on the fuel filter.

4) Diesel Engine Label Sheet - Place 744667 adjacent to English label

5) Battery Catalogue Number - Place 52356160 adjacent to English label

6) Diesel Service 6.2L - Place 52364127 adjacent to 10149667

#### Passenger Compartment

1) Diesel Engine Start Procedure Label - Place 52351523 adjacent to English label

2) Diesel Engine Start Label - Place 52363756 (CK-G-P) adjacent to English label

#### Trunk

1) Diesel Fuel Only Label - Place 746686 over English label

III. VEHICLES AFFECTED: 1992 Light Duty Trucks ---------------------------------------------- Labels are pressure sensitive; therefore, surfaces must be clean, dry, warm and free of contaminants, before labels are affixed. Labels must be pressed firmly over the entire surface.

Locate labels next to English labels, unless otherwise noted. Both labels should be readable.

#### Engine

1) Fan Caution Label - If vehicle is equipped with an English label, place 52350076 over it. This applies to RVP Truck, G-Van, M-Van, L-Van, ST Truck - Place label 52355271 adjacent to English label on: RVP Truck. - Place 52362522 and 52362525 adjacent to English label on Tracker

2) Battery Caution Labels - Place 52363359 for battery No. 1981733 on RVP, G-Van, CK- Truck - Place 52363360 for battery No. 1981734 on RVP, G-Van, M-Van, L-Van, ST-Truck, CK-Truck - Place 52363361 for battery No. 198730 on RVP-Truck, ST-Truck, CK-Truck - Place 52363362 for battery No. 198735 on RVP-Truck - Place 52366338 over English label on Pickup and Trooper

3) Battery Charge Indicator Label - Place 52362523 on: Tracker

4) Coolant Service Notice Label - Place 52356343 adjacent to English Language Label on: Isuzu Pickup and Trooper Truck.

5) Air Conditioner Compressor/Evaporator Label - Place 744775 over the words "Refrigerant Oil, Model No.", such that LH edge of overlay is even with LH edge of silver portion of compressor label on RVP-Truck, G-Van, M-Van, L- Van, ST-Truck. - Place label 744775 adjacent to corresponding English label on compressor on RVP-Truck, G-Van, M-Van, L-Van, ST-Truck. - Place label 744775 adjacent to corresponding English label on evaporator on RVP-Truck, G-Van, M-Van, L-Van, ST-Truck.

6) Air Cleaner Labels - Place 52356340 over existing English label (Pickup and Trooper Trucks).

7) Hood Prop Rod Label - Place label 52354520 over original English label on M-Van, L Van, ST-Truck.

8) Engine Oil fill Cap Label - Place label 52355864, 52355865 over original English label on the oil fill cap (key on type of oil required) on RVP-Truck, G-Van, M-Van, L-Van, ST-Truck, CK-Truck.

9) Accessory Belt Routing Label - Use 52356812 in place of 10045371 on: RVP-Truck, G-Van, CK- Truck - Use 52356813 in place of 10045372 on: RVP-Truck, G-Van, CK- Truck - Use 52356814 in place of 10045326 on: G-Van, M-Van, L-Van, CK-Truck - Use 52360932 in place of 10085701 on: RVP-Truck, ST-Truck - Use 52361584 in place of 10085749 on: RVP-Truck, CK-Truck - Use 52362321 in place of 10129519 on G-Van, M-Van, L-Van, CK- Truck - Use 52356184 in place of 10044337 on: V-Van, L-Van, ST-Truck - Use 52362146 in place of 10129531 on: M-Van, L-Van - Use 52362145 in place of 10129530 on: M-Van, L-Van - Use 52356242 in place of 10048664 on: ST-Truck - Use 52360631 in place of 10100080 on: ST-Truck - Use 52356314 in place of 15547741 on: CK-Truck - Use 52356315 in place of 15547740 on: CK-Truck - Use 52363443 in place of 10129592 on: L-M Van - Use 52364108 in place of English label on Rodeo (LUO) - Use 52366837 in place of English label on Rodeo (LG6)

- Place bilingual label over existing English label. (If label is French language only, place adjacent to English label).

10) Refrigerant Caution Label - Place 52356341 adjacent to existing English Label. (Pickup & Trooper Trucks). - Place 52362521 and 52362524 on: Tracker.

11) Rad Caution Label - Place 52356339 over existing English Label (Pickup & Trooper Trucks)

12) Caution Hot Surface Label - Place 52361669 directly on top of English Label on ST-Truck

13) Battery Catalogue Number Label - Place 52356160 adjacent to English labels on RVP-Truck, G- Van, M-Van, L-Van, ST-Truck, CK-Truck

14) Battery and Cable Installation Label - Place 52362147 adjacent to English labels on ST-Truck

15) Caution Fuel Flammable Label (4 per vehicle) - Place 52362963 around fuel line adjacent to English labels. If no labels present do not use labels, Applies to RVP- Truck, G-Van, M-Van, L-Van, ST-Truck, CK-Truck, Isuzu Pickup, Trooper Truck, Tracker.

16) Engine Jump Start Label - Place 52364147 adjacent to English label on L-M Van

17) A/C Refrigerant Changing Procedure - Place 52364148 adjacent to English label on Rodeo

#### Passenger Compartment

1) Owner's Manual Reference Label - Place label 745765 on trailing edge of driver's door in proximity to the certification label on RVP-Truck, G-Van, M- Van, ST-Truck. - If "C,K,M,P,S,T" Truck, and equipped with camper option, place label 745765 on glove box door near the camper loading label.

2) Shock Absorber Caution Label - Place 52353504 adjacent to the English labels on the shafts of each shock absorber by raising the vehicle on a hoist on ST-Truck (4 labels)

3) Transfer Case Shift Label - Place 52350175 on LH sunvisor in down position and locate label in centre of sunvisor on RVP-Truck. - Place 52352672 on LH sunvisor in down position and locate label in centre of sunvisor on ST-Truck.

4) Dome Lamp Connector Place Label - Place 744677 on RVP-Truck.

5) Roof Rear Bolt Removal Label - Place label 746000 over English label at rear RH corner of Jimmy/Blazer equipped with hardtop cap..

6) New Engine Origin Label - Place label 746246 adjacent to corresponding English label for L25 engine on LH side door on RVP-Truck. - Place label 52351461 adjacent to corresponding English label for LR1 engine on LH side door on ST-Truck.

7) Engine Start Procedure Label - Place 52364159 adjacent to English label on G-Van (L19), CK-Truck (L19). - Place 52363700 adjacent to English label on P-Truck

8) Engine Cover Removal Label - Place label 52354517 over existing English label in glove compartment area on M-Van and L-Van.

9) Childproof Lock Label - Place 52362462 adjacent to English label on Trooper Truck.

10) Utility Vehicle Handling - Place label 52354648 adjacent to existing English label on C/K-Truck, ST-Truck.

11) Dual Mode Retractor Child Restraint Seat Belt Label - Place 20584675 around belt at stitching on ST-Truck, Tracker (2 per job)

12) 4 X 4 Transfer Case Info. Label - Place 52364152 adjacent to English label on Pickup, Trooper and Rodeo.

13) Commercial Trailering Label - Place label 52355329, 52355330 or 52355331 adjacent to English label with corresponding weight on: RVP Trucks.

14) Unleaded Fuel Dash Label - Place 52356603 on top of English label on Trooper Truck.

15) Folding 2nd Seat Instruction Label - Place 52356601 adjacent to existing English label (DLX Trim) on Trooper Truck - Place 52356624 adjacent to existing English label (LS Trim) on Trooper Truck

16) Four Wheel Drive Instruction Label - Place 52356600 adjacent to existing English label on Trooper.

17) Windshield Washer Instruction - Place 52356344 over existing English Label (Pickup) - Place 52356598 over existing English label (Trooper).

18) Electrical Ground Strap Label - Place 52362148 adjacent to English label on P Truck.

19) Caution Washer Solvent Label - Place 52362752 on rear washer container on Trooper.

20) Anti-Lock Brake System - Place 52362999 on M-Van, L-Van, ST-Truck.

21) Park Brake Oper. Inst. - Place 52363416 adjacent to 15638160 on G-Van

#### Trunk

1) Jack Assembly Caution Label - Place 746125 on opposite side to English Label on jack assembly on RVP-Truck, G-Van - Place 52355476 on opposite side to English label on jack assembly on RVP-Truck - Place 52354513 on opposite side to English label on jack assembly on M-Van, L-Van - Place 52351773 on opposite side to English label on jack assembly on ST-Truck - Place 52362138 on opposite side to English label on jack assembly on CK-Truck - Place 52362520 on opposite side to English label on jack assembly on Tracker

2) Jack Instruction Label - Place 52362825 on opposite side to English on RVP-Truck - Place 52354518 over bottom section of label 52354519 on G-Van - Place 52362529 on opposite side to English on G-Van - Place 52362937 on opposite side to English on M-Van, L-Van - Place 52360257 on opposite side to English on ST-Truck - Place 52360258 on opposite side to English on ST-Truck - Place 52362611 on opposite side to English on ST-Truck - Place 52362623 on opposite side to English on CK-Truck - Place 52362587 on opposite side to English on CK-Truck - Place 52356342 on opposite side to English on Isuzu Pickup - Place 52356597 on opposite side to English on Trooper Truck - Place 52352519 on opposite side to English on Tracker

3) Light Support Caution Label - Place 52362144 on adjacent to English label on ST-Truck (3 per vehicle

4) Tailgate Opening Label - Place 52356599 adjacent to existing label on Trooper

5) Tailgate Pull Label - Place 52356602 over top of existing English label on Trooper

6) Lock Free Label - Place 52356788 adjacent to English label on Trooper Truck

7) Caution Fuel Spray Label - Place 52362319 on adjacent to English label on RVP-Truck.

IV. VEHICLES AFFECTED: 1992 Medium Duty Truck (C5-6-7, W4-5-7) --------------------------------------------------------------- Labels are pressure sensitive; therefore, surfaces must be clean, dry, warm and free of contaminants, before labels are affixed. Labels must be pressed firmly over the entire surface.

Locate labels next to English labels, unless otherwise noted. Both labels should be readable.

#### Engine Compartment

1) Battery - Place bilingual battery labels over existing labels as indicated - 52363361 over 1981730 - 52363360 over 1981734 - 52363362 over 1981735 - 52363367 over 1981736 - 52363359 over 1981733

2) Fan Blades - Place 52364320 over existing English only label on W Trucks

3) Caution - Never Open Hot (on Surge Tank Top) - Place 52364362 over existing English only label on W Trucks

4) Ether Start Notice Label - Place 52363112 adjacent to English label on C5-6-7 Truck

5) Notice Engine Start Fluids - Place 52364315 over existing English only label on W Trucks

6) Clutch Caution Tag (on Bell Housing) - Place 52363051 adjacent to English only label

7) Notice Replace Air Filter Element (W4-5-7) - Place 52364363 adjacent to existing English label

8) Notice Use DOT 3 Only (W4-5-7) - Place 52364357 over existing English English label

#### Passenger Compartment

1) Diesel Start Fluid Warning Label (C5-6-7) - Place 52363052 adjacent to English label on SIS

2) Diesel Engine Start Procedure (C5-6-7) - Place 52363058 adjacent to English label on SIS

3) Daytime Running Lights (C5-6-7) - Place 52362143 over existing English only label

4) 2-Speed Rear Axle Shift Label (C5-6-7) - Place 52363112 adjacent to existing English label 2011705

5) Roof Vent Inst. (W4-5-7) - Place 52364317 adjacent to existing English label (on vent)

6) Rear Axle Operations Label (C5-6-7) - Place 52363054 adjacent to existing English label 15504240

7) Engine Start Procedure - Place 52364353 (W7) adjacent to English label - Place 52364354 (W4) adjacent to English label - Place 52364355 (W5) adjacent to English label

8) Notice Park Brake - Place 52364319 adjacent to existing English label

9) Transmission Shift Inst. Labels (C5-6-7 Trucks) - Place 52363057 adjacent to 20181231 - Place 52363059 adjacent to 703199 - Place 52363050 adjacent to 15504169 - Place 52363053 adjacent to 716500 - Place 52363113 adjacent to 703198 - Place 52363055 adjacent to 15630600

Other Locations (Outside Surfaces, Frame Rails, etc.) ------------------------------------------------------ 1) Notice Water Separator (W4-5-7) - Place 52364358 adjacent to existing English only label

2) Notice Transmission Fluid (W4-5-7) - Place 52364321 over top of existing English only label

3) Caution-Tilt Cab (Rr of Cab O/S Lt Side) (W4-5-7) - Place 52364322 over existing English label

4) Caution Tilt Cab (W4-5-7) - Place 52364356 adjacent to existing English label

5) Lock (on Cab Supt) (W4-5-7) - Place 52364318 over existing English label

6) Avoid Drilling Label (on frame rail) (C5-6-7) - Place 52362153 over existing English label

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.