For 1990-2009 cars

## Wheel Speed Sensor Jumper Harness Replacement Front

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the connector from the front wheel speed sensor.
3. Remove the harness attaching clips (2) from the control arm (3) and the splash shield (1).
4. Lower the vehicle.
5. Remove the harness attaching clips from the strut tower.
6. Cut the wheel speed sensor wiring circuits within the main engine harness.
7. Strip the insulation on the engine harness leads and the new wheel speed sensor harness leads.

### Installation Procedure

1. Splice the sleeve provided in the jumper harness kit over each engine harness lead.
2. Install the new wheel speed sensor harness leads to the engine harness leads and crimp the connections. Verify that the wire colors match.
3. Heat shrink the tube lightly in order to seal the connection.
4. Install the harness attaching clip to the strut tower.
5. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
6. Install the harness attaching clips (2) to the control arm (3) and to the splash shield (1).
7. Install the connector to the front wheel speed sensor.
8. Lower the vehicle.
9. Perform the Diagnostic System Check .

## Wheel Speed Sensor Jumper Harness Replacement Rear

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Disconnect the two rear wheel speed sensor electrical connectors (3) from the rear wheel bearing and the speed sensor assemblies (2).
3. Disconnect the rear axle harness electrical connector between the body and the ABS and fuel sender connector.
4. Remove the rear axle harness retainers (1).
5. Remove the rear axle harness from the vehicle.

### Installation Procedure

1. Install the rear axle harness to the vehicle.
2. Install the rear axle harness retainers (1).
3. Connect the rear axle harness electrical connector between the body and the ABS and fuel sender connector.
4. Connect the two rear wheel speed sensor electrical connectors (3) to the rear wheel bearing and the speed sensor assemblies (2).
5. Lower the vehicle.
6. Perform the Diagnostic System Check .