For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Disable the SIR system. Refer to Disabling the SIR System in SIR.
3. Use a blunt tool in order to unsnap the deck lid switch (2) from the instrument panel (1).
4. Disconnect the electrical connector from the deck lid switch.

### Installation Procedure

1. Connect the electrical connector to the deck lid switch.
2. Install the deck lid switch (2) into the instrument panel (1).
3. Enable the SIR system. Refer to Enabling the SIR System in SIR.
4. Connect the negative battery cable.