For 1990-2009 cars

• | Inspect for a lack of lubrication in ball joints and tie rod ends.

• | Inspect for bind in ball joints.

• | Inspect for bind in steering column.

• | Inspect for unbalanced valve and pinion.

• | Inspect the rack bearing preload.

• | Inspect the intermediate shaft binding on the steering gear.

• | Inspect for a mispositioned intermediate shaft boot.

• | Inspect the wheel alignment.