For 1990-2009 cars

# INFO. ON INSTALLATION OF FIXED MAST ANTENNAS

********************************************************************** INFORMATION **********************************************************************

#### SUBJECT: INSTALLATION OF FIXED MAST ANTENNAS

#### MODELS: 1994 BUICK CENTURY, ROADMASTER, PARK AVENUE, LESABRE, SKYLARK, REGAL 1994 CHEVROLET CAPRICE, CAMARO, CAVALIER, CORSICA, BERETTA, LUMINA 1994 OLDSMOBILE CUTLASS CIERA, NINETY EIGHT, EIGHTY EIGHT, ACHIEVA, CUTLASS SUPREME 1994 PONTIAC FIREBIRD, BONNEVILLE, SUNBIRD, GRAND AM, GRAND PRIX

1994 CHEVROLET C/K, M/L, G AND S/T TRUCKS 1994 OLDSMOBILE BRAVADA

WARRANTY DATA HAS SHOWN THAT MANY MAST ANTENNAS ARE BEING IMPROPERLY INSTALLED DURING NVI/PDI. THIS CAN LEAD TO LOSS OF THE ANTENNA, OR DAMAGE IN CAR WASHES. USE OF THE FOLLOWING PROCEDURE WILL INSURE THAT THE MAST ANTENNA IS CORRECTLY INSTALLED.

INSTALL THE MAST ANTENNA FINGER TIGHT ON THE MOUNTING STUD. THEN, USING AN ADJUSTABLE WRENCH, TURN THE BASE OF THE ANTENNA 1/4 TURN, BEING CAREFUL NOT TO DAMAGE THE FINISH.

AN ADJUSTABLE WRENCH IS RECOMMENDED BECAUSE THE VARIATION IN THICKNESS OF PAINT ON THE BASE MAKES A SIZED WRENCH MORE LIKELY TO DAMAGE THE PAINT ON THE MAST ANTENNA BASE.

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.