For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 |

1. Use a test lamp in order to backprobe the left front door lock switch connector between terminal A and ground.
2. Press and hold the left front door lock switch in the UNLOCK position.

Does the test lamp light?

--

Go to Step 2

Go to Step 3

2 |

1. Use a test lamp in order to backprobe the left IP junction block between terminal A5 of connector C3 and ground.
2. Press and hold the left front door lock switch in the UNLOCK position.

Does the test lamp light?

--

Go to Step 4

Go to Step 5

3 | Replace the left front door lock switch. Refer to Door Lock Switch Replacement . Is the repair complete? | -- | Go to Power Windows System Check | --
4 | Replace the left IP junction block. Refer to Relay/Fuse Center Replacement . Is the repair complete? | -- | Go to Power Windows System Check | --
5 | Repair the open in CKT 194 between the left IP junction block and the left front door lock switch. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Windows System Check | --