For 1990-2009 cars

# SERVICE MANUAL UPDATE/FORCE BALANCER TORQUE PROCEDURE

1987-88 CUTLASS CIERA AND CALAIS MODELS WITH 2.5L (VIN CODE R, U) ENGINES

#### VEHICLE APPLICATIONS:

1987 Calais Models With 2.5L Engine (VIN Code U) and Manual Transaxle 1988 Cutlass Calais Models With 2.5L Engine (VIN Code U) and Automatic or Manual Transaxle 1988 Cutlass Ciera Models With 2.5L Engine (VIN Code R) and Automatic or Manual Transaxle

A revised bolt tightening procedure has been developed to provide a more uniform clamp load on the balancer assembly.

The following procedure supersedes the existing service procedure. Use J 36660 Torque Angle Meter, refer to Figure 1.

1. Snug bolts to l2 N m (9lbs.ft.) in the following sequence: 3-1-2-4.

2. Following the same sequence, tighten the short bolts (No. 2 and 1, Figure 1) to 20 N-m (15 lbs. ft.) plus 600 and the long bolts (No. 3 and 4, Figure 1) to 15 N-m (11 lbs. ft.) plus 90DEG.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.