For 1990-2009 cars

Angle | Alignment Specifications | Tolerance
--- | --- | ---
Front Caster | 3.20-5.20 Degrees | 3.20-5.20 Degrees
Front Camber | -1.30 to +0.70 Degrees | -1.30 to +0.70 Degrees
Individual Toe | 0.05 Degrees | -0.07 to +0.17 Degrees
Measure the above Toe angles with the steering wheel at level position, visually aligned with the column.
Sum Toe | 0.10 Degrees | -0.15 to +0.35 Degrees
Cross Camber | 0.70 Degrees | -1.00 to +1.00 Degrees
(Slight Cross Camber specification differences can be made when servicing the vehicle for steering pull.)
Cross Caster | 1.00 Degrees | -1.00 to +1.00 Degrees
Rear Camber | -1.05 to +0.45 Degrees | -0.75 to +0.30 Degrees
Rear Sum Toe | 0.06 Degrees | -0.26 to +0.14 Degrees
Rear Thrust Angle | -0.20 to +.20 Degrees | -0.20 to +0.20 Degrees