For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Depressurize the fuel system. Refer to Fuel Pressure Relief Procedure in Engine Controls - 3.1L.

Drain the cooling system. Recover the cooling system. Refer to Cooling System Draining and Filling and Flushing in Engine Cooling.

3. Remove the cylinder head. Refer to Cylinder Head Replacement .
4. Remove the oil pan. Refer to Oil Pan Replacement .
5. Mark the piston with the number of the cylinder from which it is being removed.
6. Mark the connecting rod and the rod cap so that they can be assembled correctly.
7. Turn the crankshaft to bottom dead center.
8. Clean the carbon from the top end of the cylinder.
9. Remove the connecting rod cap.

### Installation Procedure

#### Tools Required

J 8037 Universal Piston Ring Compressor

J 23600-B Torque Angle Meter

1. Lubricate the cylinder wall. Lubricate the piston rings. Use clean engine oil.
2. Turn the crankshaft to bottom dead center.
3. Install the connecting rod stud thread protector.

Notice: Guide the lower connecting rod end carefully to avoid damaging the crankshaft journal.

4. Install the J 8037 .

Important: Ensure that the arrow on the top of the piston faces towards the front of the engine. The flattened piston pin boss on the bottom of the piston faces the rear.

5. Install the piston and connecting rod assembly.
6. Remove the thread protectors.
7. Install the connecting rod bearing.

Important: Carefully tap the bearing cap into place with a suitable tool. Do not pull the cap down with the cap bolts or nuts.

8. Seat the bearing caps.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

9. Install the connecting rod bearing cap nuts.

Tighten
Tighten the connecting rod bearing cap nuts to 20 N·m (15 lb ft). Use the J 36660-A in order to tighten the nuts an additional 75 degrees.

10. Check the connecting rod(s) for binding. Pry the rod back and forth with a suitable tool. Loosen the bearing cap if the rod binds. Measure the connecting rod side clearance.
11. Retighten the bearing cap.
12. Install the oil pan. Refer to Oil Pan Replacement .
13. Install the cylinder head. Refer to Cylinder Head Replacement .
14. Fill the cooling system. Refer to Cooling System Draining and Filling and Flushing in Engine Cooling.
15. Connect the negative battery cable.