For 1990-2009 cars

# GRINDING OR GROWLING NOISE IN PARK ON AN INCLINE

TRANSMISSION APPLICATIONS: SUBJECT:

3T40, 4T60 GRINDING OR GROWLING NOISE IN PARK ON INCLINE

TRANSMISSION MODELS: VEHICLE APPLICATIONS:

1980-91 A,C,E,H,J,K,L,N,P,W,X AND U-VANS W/3T40,4T60

#### Bulletin Covers:

Owners of some vehicles equipped with HYDRA-MATIC 3T40 and 4T60 transaxles may comment on a grinding and/or growl noise that is noticeable when shifting the transaxle into the "Park" range on an incline. As stated in the vehicles' Owners Manual, the customer is asked to perform the following steps in sequence whenever "Parking" a vehicle equipped with a HYDRA-MATIC transmission.

1. Hold the regular brake pedal down with your right foot and apply the parking brake all the way. Follow the Parking Brake instructions in this manual for your car.

2. To move the shift lever into "P" (PARK)--

3. Pull the lever toward you and pull it up as far as it will go. If the vehicle is console equipped, hold in the button on the lever and push the lever all the way toward the front of the vehicle from you into park.

4. If you don't have to leave the engine running (briefly):

- Move the ignition key to lock or

- Depress the key release lever and move the ignition key to lock.

- Remove the key and take it with you.

5. Before you leave the driver's seat, check that your car is in park by trying to pull the shift lever out of "P" (PARK) by pulling the shift lever down without pulling it toward you (Console equipped: pull lever toward you without pressing button on the lever). If you can do this, it means that the shift lever wasn't fully locked into "P" (PARK). Or check that your car is in park by pocketing the key. If you can remove the key, the car is in "P" (PARK).

Refer the customer to the appropriate Owners Manual for additional details and instructions.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.