For 1990-2009 cars

## Instrument Panel Accessory Trim Plate Replacement Chevrolet

### Removal Procedure

1. Remove the ignition key trim cover. Pry off the cover with a flat bladed tool.
2. Gently pull the plate (1) rearward in order to disengage the retainers from the instrument panel (2).
3. Disconnect the cigarette lighter (3) connector.
4. Disconnect the cigarette lighter (2) electrical connector.
5. Remove the trim plate (1).

### Installation Procedure

1. Connect the cigarette lighter (3) electrical connector.
2. Align the trim plate tabs (1) to the instrument panel (2).
3. Snap the plate (1) into place.
4. Install the ignition key trim cover. Ensure that the unit is retained.

## Instrument Panel Accessory Trim Plate Replacement Oldsmobile

### Removal Procedure

1. Remove the ignition key trim cover. Pry off the cover with a flat bladed tool.
2. Gently pull the plate (1) rearward in order to disengage the retainers from the instrument panel (2).
3. Disconnect the cigarette lighter (3) connector.
4. Remove the plate (1).

### Installation Procedure

1. Connect the cigarette lighter (3) connector.
2. Align the trim plate (1) tabs to the instrument panel.
3. Snap the plate (1) into place.
4. Install the ignition key trim cover. Ensure that the unit is retained.