For 1990-2009 cars

## Instrument Cluster Trim Panel Replacement Chevrolet

### Removal Procedure

1. Disable the SIR system. Refer to Disabling the SIR System in SIR.
2. Remove the screws (5) from the cluster trim plate (1).
3. Gently pry out the cluster trim plate (1).
4. Disconnect the electrical connector (3) from the instrument panel lamp dimmer .
5. Disconnect the hazard warning switch (4).
6. Remove the cluster trim plate (1).

### Installation Procedure

1. Connect the hazard warning switch (4).
2. Connect the electrical connector (3) from the instrument panel lamp dimmer.
3. Align the cluster trim plate (1) tabs to the retainers.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the screws (5) to the cluster trim plate (1).

Tighten
Tighten the screws to 2 N·m (18 lb in).

5. Enable the SIR system. Refer to Enabling the SIR System in SIR.

## Instrument Cluster Trim Panel Replacement Oldsmobile

### Removal Procedure

1. Disable the SIR system. Refer to Disabling the SIR System in SIR.
2. Remove the accessory trim plates. Refer to Instrument Panel Accessory Trim Plate Replacement .
3. Remove the screws (3) from the cluster trim plate (1).
4. Gently pry out the cluster trim plate (1) from the instrument panel (2).

### Installation Procedure

1. Install the cluster trim plate (1) to the instrument panel (2).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the screws (3) to the trim plate (1).

Tighten
Tighten the screws to 2 N·m (18 lb in).

3. Install the accessory trim plates. Refer to Instrument Panel Accessory Trim Plate Replacement .
4. Enable the SIR system. Refer to Enabling the SIR System in SIR.