For 1990-2009 cars

# Cold Air Enters Vehicle Around Door Handles (Install Seal)

Subject: | Cold Air Enters Vehicle Around Door Handles (Install Seal)

Models: | 1997-2000 Chevrolet Malibu

| 1997-1999 Oldsmobile Cutlass

### Condition

Some customers may comment that cold air enters the vehicle around the door handles.

### Correction

Remove the door handle escutcheon and install an inside handle door seal with the arrow pointing up (the backside shows L for left and R for right). Make sure to tuck the lower end of the seal under the door trim pad.

### Parts Information

Part Number | Description
--- | ---
22619112 | Cold Air Seal, Inside Handle - RH Front & Rear
22619113 | Cold Air Seal, Inside Handle - LH Front & Rear

Parts are currently available from GMSPO.

### Warranty Information

For vehicles repaired under warranty, use:

Labor Operation | Description | Labor Time
--- | --- | ---
C4913 | Cold Air Seal - All Four Doors | 0.4 hr*
*This is a unique labor operation number to be used only with this bulletin. It will not be published in the Labor Time Guide Book.