For 1990-2009 cars

## Instrument Panel Storage Compartment Replacement Chevrolet

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Disable the SIR system. Refer to Disabling the SIR System in SIR.
3. Remove the accessory trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement .
4. Unsnap the center compartment (3) from the instrument panel (1).
5. Remove the compartment.

### Installation Procedure

1. Snap the center compartment (3) to the instrument panel (1). Ensure that the unit is retained.
2. Install the accessory trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement .
3. Enable the SIR system. Refer to Enabling the SIR System in SIR.
4. Connect the negative battery cable.

## Instrument Panel Storage Compartment Replacement Oldsmobile

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Disable the SIR system. Refer to Disabling the SIR System in SIR.
3. Remove the accessory trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement .
4. Remove the screws.
5. Remove the center compartment (3).
6. Disconnect the electrical connector.

### Installation Procedure

1. Connect the electrical connector.
2. Install the center compartment (3).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the screws.

Tighten
Tighten the screws to 2 N·m (18 lb in).

4. Install the accessory trim plate. Refer to Instrument Panel Accessory Trim Plate Replacement .
5. Enable the SIR system. Refer to Enabling the SIR System in SIR.
6. Connect the negative battery cable.