For 1990-2009 cars

### Removal Procedure

Caution: In order to Reduce the Risk of Fire and Personal Injury:

• | If nylon fuel pipes are nicked, scratched or damaged during installation, Do Not attempt to repair the sections of the nylon fuel pipes. Replace them.

• | When installing new fuel pipes, Do Not hammer directly on the fuel harness body clips as it may damage the nylon pipes resulting in a possible fuel leak.

• | Always cover nylon vapor pipes with a wet towel before using a torch near them. Also, never expose the vehicle to temperatures higher than 115°C (239°F) for more than one hour, or more than 90°C (194°F) for any extended period.

• | Before connecting fuel pipe fittings, always apply a few drops of clean engine oil to the male pipe ends. This will ensure proper reconnection and prevent a possible fuel leak. (During normal operation, the O-rings located in the female connector will swell and may prevent proper reconnection if not lubricated.)

Notice: Replace the EVAP pipes and hoses with the original equipment or parts that meet the GM specifications for those parts. The replacement EVAP pipe must have the same type of fittings as the original pipe in order to ensure the integrity of the connection. When replacing EVAP hoses, use only reinforced fuel-resistant hose identified with the word Fluoroelastomer or GM 6163-M on the hose. The inside hose diameter must match the outside pipe diameter. Do not use rubber hose within 100 mm (4 in) of any part of the exhaust system or within 254 mm (10 in) of the catalytic converter.

1. Remove the retaining hardware and the clamp as necessary.
2. Note the location and the position for future reference.
3. Inspect the hoses and the vapor lines for cuts, swelling, cracks, kinks and distortion.
4. Remove the pipe or the hose.

### Installation Procedure

Important: Follow the same routing as original pipe or hose.

1. Reinstall the vapor line or hose.
2. Reinstall the retaining hardware and clamps.