For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 6627-A Wheel Stud Remover

1. Raise the vehicle on a hoist. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the wheel and tire assembly. Refer to Wheel Removal in Tires and Wheels.

Notice: Do not hammer on brake drum as damage to the bearing or deformation of the drum could result.

3. Remove the brake drum. Refer to Brake Drum Replacement in Drum Brakes.
4. Remove the wheel stud (2) using the J 6627-A .
5. Dispose of the stud (2).

### Installation Procedure

1. Install a new stud. Insert the stud from the back side of the hub.
2. Install 4 flat washers (1) on the stud.
3. Install the wheel nut (2) with the flat side toward the washers (1).
4. Tighten the nut (2) until the stud head is properly seated in the hub flange.
5. Remove the nut (2) and washers (1).
6. Install the brake drum. Refer to Brake Drum Replacement in Drum Brakes.
7. Install the wheel and tire assembly. Refer to Wheel Installation in Tires and Wheels.