For 1990-2009 cars

### Removal Procedure

1. Remove the steering lever. Refer to Tilt Lever Replacement - On Vehicle in Steering Wheel and Column - Tilt.
2. Remove the steering column upper and lower covers. Refer to Steering Column Trim Cover Replacement - On Vehicle in Steering Wheel and Column - Tilt.
3. Disconnect the hazard warning switch electrical connector.
4. Remove the hazard warning switch from the trim plate.

### Installation Procedure

1. Install the hazard warning switch from the trim plate.
2. Connect the hazard warning switch electrical connector.
3. Install the steering column upper and lower covers. Refer to Steering Column Trim Cover Replacement - On Vehicle in Steering Wheel and Column - Tilt.
4. Install the steering lever. Refer to Tilt Lever Replacement - On Vehicle in Steering Wheel and Column - Tilt.