For 1990-2009 cars

# SMU - SECTION 6A2 - ENGINE MECHANICAL

#### SUBJECT: SERVICE MANUAL UPDATE--SECTION 6A2-ENGINE MECHANICAL- CAMSHAFT REAR COVER BOLT TORQUE SPECIFICATION

#### MODELS: 1993-96 BUICK CENTURY 1990-96 CHEVROLET BERETTA, CAVALIER, CORSICA 1993-96 OLDSMOBILE CUTLASS CIERA 1990-93 PONTIAC TEMPEST (GM OF CANADA ONLY) 1995-96 PONTIAC SUNFIRE

1994-96 CHEVROLET AND GMC S MODELS WITH 2.2L ENGINE (VINS G, 4--RPOS LM3, LN2)

THE CAMSHAFT REAR COVER BOLT TORQUE WAS OMITTED FROM SOME OF THE SERVICE MANUALS.

CAMSHAFT REAR COVER BOLT TORQUE SPECIFICATION: THE TORQUE SPECIFICATION FOR THE CAMSHAFT REAR COVER IS 12 N.M (106 LB. IN.).

FIGURES: 0 ATTACHMENTS: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1996. GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.