For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Door Trim Panel Replacement .
2. Remove the remote control from the outside rearview mirror remote control bezel (manual only).
3. Disconnect the power mirror wire harness (power only).
4. Remove the front door inner panel mirror insulator (3).
5. Remove the outside rearview mirror nuts (2).
6. Remove the outside rearview mirror (1).

### Installation Procedure

1. Install the outside rearview mirror.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the outside rearview mirror nuts (2). Tighten the nuts in the following order:

2.1. | Top

2.2. | Forward

2.3. | Rear

Tighten
Tighten the nuts to 10 N·m (89 lb in).

3. Install the front door inner panel mirror insulator (3).
4. Connect the power mirror wire harness (power only).
5. Install the remote control to the outside rearview mirror remote control bezel (manual only).
6. Install the door trim panel. Refer to Door Trim Panel Replacement .