For 1990-2009 cars

# MANUAL UPDATE-SECTION 6E DRIVEABILITY AND EMISSION

#### MODELS/YEARS 1989 3300 (VIN N) CUTLASS CIERA AND CUTLASS CALAIS MODELS

Several instances of alternate wire colors going to the C31 module on 1989 Cutlass Ciera and Cutlass Calais vehicles equipped with a 3300 (VIN N) engine have been reported. This would effect wire colors on diagnostic Charts A-3, C-4H-1, C-4H-2, and Code 42 Chan found in Section 6E "Driveability and Emissions' of the Service Manual. It would also effect the wire colors on the ECM Wiring Diagrams at the front of Section 6E3-A "Driveability and Emissions" and Section 8A "Electrical Diagnosis", page 8A-21 -1.

On vehicles that have the alternate wire colors, the circuits remain the same. If the colors do not match that of the Service Manual, they may be as follows:

C31 Circuit Connector Number Original Color Alternate Color --------- ------ -------------- --------------- A 423 WHT WHT B 424 TAN/BLK TAN/BLK c 430 PPL/WHT PPL/WHT D 453 BLK/RED BLK/RED E 121 WHT WHT F 646 LT BLU/WHT WHT/BLK G 645 GRY/RED DK BLU/WHT H 644 WHT/BLK LT BLU/WHT K 643 DK BLU/WHT GRY/RED Cutlass Calais only M 239 PNK/WHT PNK/BLK Cutlass Ciera only M 839 PNK/WHT PNK/BLK

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.